

**LAB-05**


**Implement the following VLAN scenario in eNSP simulator:**


**eNSP simulation:**


****


VLAN CONFIGURATION ON LSW1:

ROUTER CONFIGURATION:




PING PC4 FROM PC1 (Different VLAN’s)

PING PC4 FROM PC3 (same VLAN’s)

PING PC3 FROM PC2 (Different VLAN’s)

PING PC1 FROM PC3 (Different VLAN’s)



PING PC1 FROM PC2 (same VLAN’s)

